Accessing Customer Service Menu

- Press the MENU button on the remote control.

- Choose ‘Setup’, and press the Centre button.

- Press RED button and within 3 seconds press the Centre button.

- Choose ‘Settings’, and press the Centre button.

|  |  |
| --- | --- |
| SETTINGS | |
| CLOCK | [ON /OFF] |
| CLOCK TIMEOUT | [0 – 65535] |
| AUTO ST.BY 15 MIN. | [ON / OFF] |
| TELETEXT LANGUAGE | 00-06 (Default value according to actual country setting) |
| B&O NETWORK DOMAIN |  |
| **REROUTE LIGHT/CONTROL** | **[YES /NO]** |
| HbbTV | [ON /OFF] |
| RESET TO DEFAULT |  |
| RESET CI+ AUTHENTICATIONS |  |

**REROUTE LIGHT/CONTROL** (to Master Link Gate Way) can be ON/OFF

- Can be set ON for enabling reroute of all LIGHT and CONTROL commands from remote to MLGW.  
 If this menu offers multiple choices, then select **'mlgw'**

- It is recommended only to have **one product in a room with this setting.**

- Three or more products in a room can cause fail on ML

Settings is **default ON**

In Power Settings, Standby menu make one or two Quick-Start Timer(s) covering the period(s) where you want to be able to use the integration between BeoVision 11 and MLGW.