# 2 Test functions controlled via IR.

## 2.1 General rules.

Control must be made by a one-way remote control (BL1000, Beo4 or Beo5).

To access a test function, the Beolink Active or Beolink Passive must be in standby mode.

With the STOP command or by local operation, the chosen test function can be skipped anytime.  
By entering an illegal command or a numeric value outside the area, the current test function is left in the same way as with the STOP command

## 2.3 Setup about Light/Control Reroute On/Off

**Purpose**:

To Enable or Disable the function:

Reroute all LIGHT and CONTROL commands to ML

This function is used if 3rd party system is to be controlled by B&O remote through Beolink Active or Beolink Passive and MasterLink GateWay (MLGW)

Only one (max. two) products in a room must have this setting to ON.

Three or more products with this setting to ON in same room,

can cause jamming/delays/malfunction on ML !!!

Keypress. Comments

-------------------------------------------------------------------------------------------------------------------------

[MENU]   
[0]   
[5]  
[GO] Set-up mode entered.

Function is default OFF.

[^] Reroute LIGHT and CONTROL to ML **enabled**.

[v] Reroute LIGHT and CONTROL to ML **disabled**.

[GO] Setting stored.

Confirm by blink with LED (like Option prog.)

-------------------------------------------------------------------------------------------------------------------------

# 