# 2 Test functions controlled via IR.

## 2.1. General rules.

Control must be made by a one-way remote control (BL1000, Beo4 or Beo5)

To access a test function, the BeoLab 3500 must be in standby mode.

With the STOP command or by local operation, the chosen test function can be skipped anytime.
By entering an illegal command or a numeric value outside the area, the current test function is left in the same way as with the STOP command.

## 2.6 Setup about Light/Control Reroute On/Off

**Purpose:**

To Enable or Disable the function:

Reroute all LIGHT and CONTROL commands to ML

This function is used if 3. Party system is to be controlled by B&O remote through BLAB3500 and MasterLink GateWay (MLGW)

Only one (max. two) products in a room must have this setting to ON.

Three or more products with this setting to ON in same room,

can cause jamming/delays/malfunction on ML !!!

Keypress. Display Comments

--------------------------------------------------------------------------------------------------------------------------

[MENU] ? 1. [MENU] opens for Wake Up Timer programming

[MENU]

[0]

[5]

[GO] "MLGW OFF" Current state displayed.

 Default OFF

[^] "MLGW ON " Reroute LIGHT and CONTROL to ML **enabled**.

[v] "MLGW OFF" Reroute LIGHT and CONTROL to ML **disabled**.

[GO] "MLGW OFF " Setting stored

[STOP] or

3 sec. timeout Exit function

--------------------------------------------------------------------------------------------------------------------------