Entering SERVICE MENU:

There are two ways to enter the service menu, either by the BeoSound 4 keyboard or the Beo4 remote control.

BeoSound 4:

- The BeoSound 4 is in Standby mode

- Press “MENU”

- Use the navigation wheel to move the pointer to Setup, and enter the Setup Menu by Pressing GO at the centre of the navigation wheel

- Press 0 0 GO to enter the SERVICE MENU

- Turn the navigation wheel to move the cursor up and down in the SERVICE MENU

- Press GO or >> to select an item in the SERVICE MENU

- Press STOP or << to return to the SERVICE MENU

Beo4 (not in Option 0):

- The BeoSound 4 is in Standby mode

- Press MENU

- Press GO to enter the SETUP MENU (be aware of the menu language setting)

- Press 0 0 GO to enter the SERVICE MENU

- Press Up or Down to move the cursor up and down in the SERVICE MENU

- Press GO or >> to select an item in the SERVICE MENU

- Press STOP or << to return to the SERVICE MENU

SERVICE MENU

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SERVICE MENU

1 SW VERSIONS

2 ERROR LIST

3 PRODUCT ID

4 PRODUCT INFO

5 SERVICE COUNTERS

6 DEFAULT SETTINGS

7 KEYBOARD TEST

8 LOADER LOCK

9 CD TEST MODES

10 DAB STATUS

11 SD/CODEC STATUS

12 DOOR SENSITIVITY

**• 13 ML GATEWAY**

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

Select 13 ML GATEWAY

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

…ML GATEWAY

1 STATUS TO MLGW OFF

2 CMDS TO MLGW OFF

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

**STATUS TO MLGW** (Master Link Gate Way) can be ON/OFF

- Shall only be **ON if status to a control panels is needed**

**CMDS TO MLGW** (Master Link Gate Way) can be ON/OFF

- Can be set ON for enabling reroute of all LIGHT and CONTROL commands from remote to MLGW.

- It is recommended only to have **one product in a room with this setting to ON**

- Three or more products in a room can cause fail on ML

Both settings are **default OFF**